1. Print or copy onto stiff paper. 2. Fold on dotted lines. 3. Cut this window out carefully. 4. Glue tab back on itself, when dry, glue halves together.

glue -- glue -- glue glue -- glue -- glue glue -- glue -- glue

(C) Copyright 1991, Andy Kinsman, P.O. Box 1457, Fairport, N.Y. 14450-1457 "Collector of Slide Rules" kinsman@ssd.kodak.com

K A B L C D

B L C

CONVERSION FACTORS LINEAR MEASURE AREA MEASURE VOLUME MEASURE WEIGHT ENERGY - WORK PRESSURE 1 inch = 2.54 cm 1 foot = 0.3048 m 1 yard = 0.9144 m 1 mile = 1.609 km 1 mile = 5280 ft 1 naut.mile = 1.152 mi.

1 sq inch = 6.452 cm2 1 sq foot = 0.0929 m2 1 sq yard = 0.8361 m2 1 sq mile = 2.59 km2 1 sq mile = 640 acres 1 acre = 43,560 sq ft

1 cu inch = 16.39 cm3 1 cu foot = 0.0283 m3 1 cu yard = 0.7646 m3 1 U.S. gallon = 3.785 liter 1 U.S. gallon = 231 cu in. 1 cu foot = 28.32 liter

1 Pound = 0.4536 kg 1 Grain = 0.0648 g 1 U.S. gallon = 8.345 lb 1 cu foot of water = 62.43 lb

1 Btu = 778 ft-lb 1 hp = 0.707 Btu/sec 1 hp = 550 ft-lb/sec 1 hp = 0.746 kw

1 atm = 14.7 psi 1 ft of water = 0.4335 psi 1 in. of mercury = 0.4912 psi 1 in. of mercury = 1.133 ft of water 1 in. of mercury = 780 ft of air

π π

.1.0 .11.0